Arduino

Reference Language | Libraries | Comparison | Changes

## constrain(x, a, b)

#### Description

Constrains a number to be within a range.

#### Parameters

x: the number to constrain, all data types

a: the lower end of the range, all data types

b: the upper end of the range, all data types

#### Returns

x: if x is between a and b

a: if x is less than a

b: if x is greater than b

#### Example

    sensVal = constrain(sensVal, 10, 150);
    // limits range of sensor values to between 10 and 150

#### See also

- min()
- max()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers