Arduino

Reference Language | Libraries | Comparison | Changes

GSM : GSM_SMS class

## peek()

#### Description

Returns the next byte (character) of an incoming SMS without removing it from the message. That is, successive calls to peek() will return the same character, as will the next call to read(). peek() inherits from the Stream utility class.

#### Syntax

SMS.peek()

#### Parameters

none

#### Returns

int - the first byte available of a SMS message (or -1 if no data is available)

#### Example

/*
SMS receiver
This sketch, for the Arduino GSM shield, waits for SMS messages
and displays them through the Serial port.
Circuit:
* GSM shield
created 25 Feb 2012
by Javier Zorzano / TD
This example is in the public domain.
*/
// libraries
#include <GSM.h>
// PIN Number
#define PINNUMBER ""
// initialize the library instance
GSM gsmAccess; // include a 'true' parameter for debug enabled
GSM_SMS sms;
char remoteNumber[20]; // Holds the emitting number
void setup()
{
// initialize serial communications
Serial.begin(9600);
Serial.println("SMS Messages Receiver");
// connection state
boolean notConnected = true;
// Start GSM shield
// If your SIM has PIN, pass it as a parameter of begin() in quotes
while(notConnected)
{
if(gsmAccess.begin(PINNUMBER)==GSM_READY)
notConnected = false;
else
{
Serial.println("Not connected");
delay(1000);
}
}
Serial.println("GSM initialized");
Serial.println("Waiting for messages");
}
void loop()
{
char c;
// If there are any SMSs available()
if (sms.available())
{
Serial.println("Message received from:");
// Get remote number
sms.remoteNumber(remoteNumber, 20);
Serial.println(remoteNumber);
// This is just an example of message disposal
// Messages starting with # should be discarded
if(sms.peek()=='#')
{
Serial.println("Discarded SMS");
sms.flush();
}
// Read message bytes and print them
while(c=sms.read())
Serial.print(c);
Serial.println("\nEND OF MESSAGE");
// delete message from modem memory
sms.flush();
Serial.println("MESSAGE DELETED");
}
delay(1000);
}
[Get Code]

#### See Also

- beginSMS()
- ready()
- endSMS()
- available()
- remoteNumber()
- read()
- write()
- print()
- peek()
- flush()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers