Arduino

Reference Language | Libraries | Comparison | Changes

## SoftwareSerial: overflow()

#### Description

Tests to see if a software serial buffer overflow has occurred. Calling this function clears the overflow flag, meaning that subsequent calls will return false unless another byte of data has been received and discarded in the meantime.

The software serial buffer can hold 64 bytes.

#### Syntax

mySerial.overflow()

#### Parameters

none

#### Returns

boolean

#### Example

#include <SoftwareSerial.h>
// software serial : TX = digital pin 10, RX = digital pin 11
SoftwareSerial portOne(10,11);
void setup()
{
// Start the hardware serial port
Serial.begin(9600);
// Start software serial port
portOne.begin(9600);
}
void loop()
{
if (portOne.overflow()) {
Serial.println("SoftwareSerial overflow!");
}
[Get Code]

#### See also

- SoftwareSerial()
- read()
- print()
- println()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers