Arduino

Reference Language | Libraries | Comparison | Changes

## Stepper(steps, pin1, pin2)

## Stepper(steps, pin1, pin2, pin3, pin4)

#### Description

This function creates a new instance of the Stepper class that represents a particular stepper motor attached to your Arduino board. Use it at the top of your sketch, above setup() and loop(). The number of parameters depends on how you've wired your motor - either using two or four pins of the Arduino board.

#### Parameters

steps: the number of steps in one revolution of your motor. If your motor gives the number of degrees per step, divide that number into 360 to get the number of steps (e.g. 360 / 3.6 gives 100 steps). (int)

pin1, pin2: two pins that are attached to the motor (int)

pin3, pin4: optional the last two pins attached to the motor, if it's connected to four pins (int)

#### Returns

A new instance of the Stepper motor class.

#### Example

Stepper myStepper = Stepper(100, 5, 6);

#### See also

- setSpeed(rpm)
- step(steps)

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers