Arduino

Reference Language | Libraries | Comparison | Changes

## Wire.endTransmission()

#### Description

Ends a transmission to a slave device that was begun by beginTransmission() and transmits the bytes that were queued by write().

As of Arduino 1.0.1, endTransmission() accepts a boolean argument changing its behavior for compatibility with certain I2C devices.

If true, endTransmission() sends a stop message after transmission, releasing the I2C bus.

If false, endTransmission() sends a restart message after transmission. The bus will not be released, which prevents another master device from transmitting between messages. This allows one master device to send multiple transmissions while in control.

The default value is true.

#### Syntax

Wire.endTransmission()
Wire.endTransmission(stop)

#### Parameters

stop : boolean. true will send a stop message, releasing the bus after transmission. false will send a restart, keeping the connection active.

#### Returns

byte, which indicates the status of the transmission:

- 0:success
- 1:data too long to fit in transmit buffer
- 2:received NACK on transmit of address
- 3:received NACK on transmit of data
- 4:other error

#### See Also

- Wire.beginTransmission()
- Wire.write()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers